,Voltage##OTHER##,V_RightEndCap##OTHER##,V_LeftEndCap##OTHER##,Product Range##OTHER##,Max Height from ceiling##LENGTH##MILLIMETERS,M_Housing##OTHER##,IfcExportType##OTHER##,IfcExportAs##OTHER##,Weekly##OTHER##,Warranty ID##OTHER##,Upward Component ##OTHER##,Unified Glare Rating ##OTHER##,Uniclass 2015##OTHER##,URL to O&M Manual##OTHER##,URL to Energy Technology List##OTHER##,Total Power##OTHER##,Total Light Output ##OTHER##,Testing method##OTHER##,Supply Phase##OTHER##,Suitable for Photocell Control##OTHER##,Suitable for Motion Detector Control##OTHER##,Suitable for Dimming ##OTHER##,Suitable Dimmer Type##OTHER##,Standards##OTHER##,Shipping Weight##OTHER##,Service life ##OTHER##,Secondary Rated Lamp Life##OTHER##,Secondary Lamp Voltage##OTHER##,Secondary Lamp International Type Code##OTHER##,Secondary Lamp Initial Lumens ##OTHER##,Secondary Lamp Included##OTHER##,Secondary Lamp Efficacy##OTHER##,Secondary Lamp Colour Temperature##OTHER##,Secondary Lamp Colour Rendering Index##OTHER##,Secondary Lamp Cap##OTHER##,Secondary Lamp##OTHER##,Responsible Sourcing of Materials##OTHER##,Responsible Extraction of Materials##OTHER##,Rated Lamp Life##OTHER##,Quarterly##OTHER##,Product Model Number##OTHER##,Product Literature##OTHER##,Primary Lamp Type##OTHER##,Power Supply Kit##OTHER##,Power Factor##OTHER##,Photocell##OTHER##,Overall Width##OTHER##,Overall Light Output Ratio##OTHER##,Overall Length##OTHER##,Overall Height##OTHER##,Output Lumens Indirect light##OTHER##,Output Lumens Direct light##OTHER##,Number of Secondary Lamps##OTHER##,Number of Primary Lamps##OTHER##,Number of Poles##OTHER##,Motion Sensor##OTHER##,Motion Detector##OTHER##,Monthly##OTHER##,Minimum Operating Temperature##OTHER##,Maximum Operating Temperature##OTHER##,Material Ingredient Reporting##OTHER##,Manufacturer Website##OTHER##,Produttore##OTHER##,Maintenance Required: 8001-12000hrs ##OTHER##,Maintenance Required: 601-1000hrs##OTHER##,Maintenance Required: 4001-8000hrs ##OTHER##,Maintenance Required: 301-600hrs ##OTHER##,Maintenance Required: 2001-4000hrs ##OTHER##,Maintenance Required: 1001-2000hrs ##OTHER##,Maintenance Required: 0-300hrs ##OTHER##,Luminance at 65deg Angle##OTHER##,Luminaire Type##OTHER##,Luminaire Maintenance Factor##OTHER##,Luminaire Cleaning Interval ##OTHER##,Louvre/Lens##OTHER##,Location of Manufacturer##OTHER##,Light Output Pattern##OTHER##,Light Fixture Mounting Type##OTHER##,Life Cycle Analysis##OTHER##,Lamp Survival Factor##OTHER##,Lamp Replacement Interval##OTHER##,Lamp Included##OTHER##,Lamp Cap##OTHER##,LED lifetime##OTHER##,LED Maintained Colour Variation        ##OTHER##,LED Initial Colour Variation                     ##OTHER##,International Type Code##OTHER##,Intended Market##OTHER##,Integral Fuse or Circuit Protection ##OTHER##,Integral Emergency Lighting Battery Type##OTHER##,Input Lumens Indirect light##OTHER##,Input Lumens Direct light##OTHER##,Initial Lumens##OTHER##,Infills##OTHER##,IP Rating##OTHER##,IK Rating##OTHER##,IES Files ##OTHER##,Housing Material##OTHER##,Housing Finish ##OTHER##,Housing Colour ##OTHER##,Hazardous Area Protection Type##OTHER##,Hazardous Area Category##OTHER##,Gross Weight##OTHER##,Green Guide for Specification##OTHER##,Frequency ##OTHER##,Fixings##OTHER##,Fire Shroud##OTHER##,Fire Rating Duration##OTHER##,Fire Rated Temperature##OTHER##,Fire Rated##OTHER##,Features##OTHER##,Face Width##OTHER##,Face Shape##OTHER##,Face Length##OTHER##,External Control Line Voltage##OTHER##,Expected Life##OTHER##,Environmental Product Declaration##OTHER##,End Caps/Transition Caps/Joints##OTHER##,Emergency light output percentage##OTHER##,Emergency Lighting Battery##OTHER##,Emergency Charging Power      ##OTHER##,Emergency##OTHER##,Embodied Carbon ##OTHER##,Efficiency##OTHER##,Earth Point ##OTHER##,ENEC Certification of European conformity##OTHER##,Duration of Integral Emergency Lighting ##OTHER##,Drive Current                                         ##OTHER##,Downward Component##OTHER##,Distance_LengthLamp##LENGTH##MILLIMETERS,Distance_LampFromCeiling##LENGTH##MILLIMETERS,Diffusing screen##OTHER##,Designed by##OTHER##,Prospetto di default##LENGTH##MILLIMETERS,Daylight Sensor##OTHER##,Daily##OTHER##,Cut Out Width##OTHER##,Cut Out Length##OTHER##,Current ##OTHER##,Control Gear Type##OTHER##,Control Gear Standby Power ##OTHER##,Control Gear Required##OTHER##,Control Gear Location##OTHER##,Column##OTHER##,Colour Temperature##OTHER##,Colour Rendering Index##OTHER##,CE Approval##OTHER##,Bespoke Timeframe##OTHER##,Beam Angle Transverse Axis ##ANGLE##DECIMAL DEGREES,Beam Angle Longditudinal Axis ##ANGLE##DECIMAL DEGREES,Basis of lifetime luminaire failures       ##OTHER##,Basis of lifetime lumen depreciation  ##OTHER##,Application Environment##OTHER##,Annually##OTHER##,Ambient Temperature                            ##OTHER##,Air Handling##OTHER##,Access Clearance Top##OTHER##,Access Clearance Right##OTHER##,Access Clearance Rear##OTHER##,Access Clearance Left##OTHER##,Access Clearance Front##OTHER##,Access Clearance Bottom##OTHER##,6 Monthly##OTHER##
A.24_Recessed_MagneticTrack_Track_1176mm_White_AQ15001,-,0,1,A.24,0.000000000000,Artemide_Aluminum_White,NOT DEFINED,IfcLightFixtureType,-,https://cloud.artemide.com/5-years-warranty,0,-,Pr_70_70_48,https://www.artemide.com/contents/documenti/prodotto/a.24_binario_magnetico_instructions4837164.zip,-,0,0,-,0,-,-,N,-,-,0,-,0,0,-,0,-,0,0,0,-,-,-,-,0,-,AQ15001,-,-,-,0,-,27,0,1176,54,0,0,0,0,0,-,-,-,0,0,-,https://www.artemide.com,Artemide,-,-,-,-,-,-,-,0,-,0,-,-,-,-,Recessed,-,-,-,N,-,0,0,0,-,Unset,-,-,0,0,0,-,IP20,-,-,Aluminium,Painted,White,-,-,6,-,0,-,-,0,0,-,-,0,Rectangular,0,0,-,-,-,0,-,0,N,0,0,-,Y,0,0,0,1176.000000000000,0.000000000000,-,Carlotta_deBevilacqua,1219.200000000000,-,-,54,1176,0,-,0,-,-,-,0,0,Y,-,0.000000000000,0.000000000000,0,0,Internal,-,0,-,0,0,0,0,0,0,-
A.24_Recessed_MagneticTrack_Track_1176mm_Black_AQ15004,-,0,1,A.24,0.000000000000,Artemide_Aluminum_Black,NOT DEFINED,IfcLightFixtureType,-,https://cloud.artemide.com/5-years-warranty,0,-,Pr_70_70_48,https://www.artemide.com/contents/documenti/prodotto/a.24_binario_magnetico_instructions4837164.zip,-,0,0,-,0,-,-,N,-,-,0,-,0,0,-,0,-,0,0,0,-,-,-,-,0,-,AQ15004,-,-,-,0,-,27,0,1176,54,0,0,0,0,0,-,-,-,0,0,-,https://www.artemide.com,Artemide,-,-,-,-,-,-,-,0,-,0,-,-,-,-,Recessed,-,-,-,N,-,0,0,0,-,Unset,-,-,0,0,0,-,IP20,-,-,Aluminium,Painted,Black,-,-,6,-,0,-,-,0,0,-,-,0,Rectangular,0,0,-,-,-,0,-,0,N,0,0,-,Y,0,0,0,1176.000000000000,0.000000000000,-,Carlotta_deBevilacqua,1219.200000000000,-,-,54,1176,0,-,0,-,-,-,0,0,Y,-,0.000000000000,0.000000000000,0,0,Internal,-,0,-,0,0,0,0,0,0,-
A.24_Recessed_MagneticTrack_Track_2352mm_White_AQ15101,-,0,1,A.24,0.000000000000,Artemide_Aluminum_White,NOT DEFINED,IfcLightFixtureType,-,https://cloud.artemide.com/5-years-warranty,0,-,Pr_70_70_48,https://www.artemide.com/contents/documenti/prodotto/a.24_binario_magnetico_instructions4837164.zip,-,0,0,-,0,-,-,N,-,-,0,-,0,0,-,0,-,0,0,0,-,-,-,-,0,-,AQ15101,-,-,-,0,-,27,0,2352,54,0,0,0,0,0,-,-,-,0,0,-,https://www.artemide.com,Artemide,-,-,-,-,-,-,-,0,-,0,-,-,-,-,Recessed,-,-,-,N,-,0,0,0,-,Unset,-,-,0,0,0,-,IP20,-,-,Aluminium,Painted,White,-,-,6,-,0,-,-,0,0,-,-,0,Rectangular,0,0,-,-,-,0,-,0,N,0,0,-,Y,0,0,0,2352.000000000000,0.000000000000,-,Carlotta_deBevilacqua,1219.200000000000,-,-,54,2352,0,-,0,-,-,-,0,0,Y,-,0.000000000000,0.000000000000,0,0,Internal,-,0,-,0,0,0,0,0,0,-
A.24_Recessed_MagneticTrack_Track_2352mm_Black_AQ15104,-,0,1,A.24,0.000000000000,Artemide_Aluminum_Black,NOT DEFINED,IfcLightFixtureType,-,https://cloud.artemide.com/5-years-warranty,0,-,Pr_70_70_48,https://www.artemide.com/contents/documenti/prodotto/a.24_binario_magnetico_instructions4837164.zip,-,0,0,-,0,-,-,N,-,-,0,-,0,0,-,0,-,0,0,0,-,-,-,-,0,-,AQ15104,-,-,-,0,-,27,0,2352,54,0,0,0,0,0,-,-,-,0,0,-,https://www.artemide.com,Artemide,-,-,-,-,-,-,-,0,-,0,-,-,-,-,Recessed,-,-,-,N,-,0,0,0,-,Unset,-,-,0,0,0,-,IP20,-,-,Aluminium,Painted,Black,-,-,6,-,0,-,-,0,0,-,-,0,Rectangular,0,0,-,-,-,0,-,0,N,0,0,-,Y,0,0,0,2352.000000000000,0.000000000000,-,Carlotta_deBevilacqua,1219.200000000000,-,-,54,2352,0,-,0,-,-,-,0,0,Y,-,0.000000000000,0.000000000000,0,0,Internal,-,0,-,0,0,0,0,0,0,-
